CUSTOMER START UP RESPONSIBILITIES

1. The facility/corporate management sign purchase agreement.

2. Have installation form completed by the facility.

3. The facility will have the injection equipment installed as follows:

 (Installation may be done by in-house engineer or an outside service.)

 A. Mount the cabinets to the wall where indicated by the information on the installation form.

 B. Attach the chemical suction tubing with probes and chemical output tubing to washer.

 C. Attach the wiring harness to the injection unit and run the cable to the washer.

 D. Install a water feed hose to the injection unit from a cold-water wall valve.

4. The laundry staff must attend training program.

5. The laundry manager will receive contact information.

6. The laundry will receive an installation/service report of the startup and an equipment loan agreement. The laundry manager will sign both papers.